
How To Upgrade Security Module


1. Remove 2 screws and connect RS232 cable.


1. Start SecureCRT.





1. Reboot device and press u to stop booting. Input 1 to enter upgrading mode.




1. Send serial.bin firmware by Ymodem option.



1. New firmware version will be shown after reboot.



[ - The End - ]